|  |  |  |
| --- | --- | --- |
| Display 7 Segments | Pin | MUX |
| A | PG0 | 0 |
| B | PG1 | 0 |
| C | PG2 | 0 |
| D | PG3 | 0 |
| E | PG4 | 0 |
| F | PG5 | 0 |
| G | PI0 | 0 |
| Dot | PI1 | 0 |

|  |  |  |
| --- | --- | --- |
| SIM900 | Pin | MUX |
| Reset | PC3 | 0 |
| LED | PC7 | 0 |
| On/Off | PC16 | 0 |
| RI | PI11 | 0 |
| RX | RX6 |  |
| TX | TX6 |  |